
T0BD0 000:300 SEGGER J-Link V4.76d Log File (0001ms, 0116ms total)
T0BD0 000:300 DLL Compiled: Sep 13 2013 16:35:06 (0001ms, 0116ms total)
T0BD0 000:300 Logging started @ 2020-03-16 14:18 (0001ms, 0116ms total)
T0BD0 000:301 JLINK_SetWarnOutHandler(...) (0000ms, 0116ms total)
T0BD0 000:301 JLINK_OpenEx(...)
Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
Hardware: V7.00
S/N: 20090928
Feature(s): RDI,FlashDL,FlashBP,JFlash,GDBFull  returns O.K. (0032ms, 0148ms total)
T0BD0 000:333 JLINK_SetErrorOutHandler(...) (0000ms, 0148ms total)
T0BD0 000:333 JLINK_ExecCommand("ProjectFile = "F:\佳显电子\新产品开发\新产品开发--合力泰电子纸\常规品\GDEH0116Zx_SSD1677-20200309\Project\JLinkSettings.ini"", ...)  returns 0x00 (0001ms, 0149ms total)
T0BD0 000:334 JLINK_ExecCommand("Device = STM32F103VE", ...)
                JLINK_AddMirrorAreaEx(Addr = 0x00000000, Size = 0x00000000) (0000ms, 0000ms total)
              Device "STM32F103VE" selected (512 KB flash, 64 KB RAM).  returns 0x00 (0002ms, 0151ms total)
T0BD0 000:336 JLINK_ExecCommand("DisableConnectionTimeout", ...)  returns 0x01 (0000ms, 0151ms total)
T0BD0 000:336 JLINK_GetHardwareVersion()  returns 0x11170 (0000ms, 0151ms total)
T0BD0 000:336 JLINK_GetDLLVersion()  returns 47604 (0000ms, 0151ms total)
T0BD0 000:336 JLINK_GetFirmwareString(...) (0000ms, 0151ms total)
T0BD0 000:336 JLINK_GetDLLVersion()  returns 47604 (0000ms, 0151ms total)
T0BD0 000:336 JLINK_GetCompileDateTime() (0000ms, 0151ms total)
T0BD0 000:336 JLINK_GetFirmwareString(...) (0000ms, 0151ms total)
T0BD0 000:336 JLINK_GetHardwareVersion()  returns 0x11170 (0000ms, 0151ms total)
T0BD0 000:336 JLINK_TIF_Select(JLINKARM_TIF_SWD)  returns 0x00 (0005ms, 0156ms total)
T0BD0 000:341 JLINK_SetSpeed(5000) (0001ms, 0157ms total)
T0BD0 000:344 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)  returns JLINKARM_RESET_TYPE_NORMAL (0000ms, 0157ms total)
T0BD0 000:344 JLINK_Reset() >0x108 TIF>Found SWD-DP with ID 0x1BA01477 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x108 TIF>Found SWD-DP with ID 0x1BA01477 >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF>
 >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>Found Cortex-M3 r1p1, Little endian. -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0)
 -- CPU_ReadMem(4 bytes @ 0xE0002000)FPUnit: 6 code (BP) slots and 2 literal slots -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_ReadMem(4 bytes @ 0xE00FF010)TPIU fitted. -- CPU_ReadMem(4 bytes @ 0xE00FF014)ETM fitted. -- CPU_ReadMem(4 bytes @ 0xE00FF018) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC) >0x35 TIF> -- CPU is running
 -- CPU_WriteMem(4 bytes @ 0xE000ED0C) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000) (0106ms, 0263ms total)
T0BD0 000:450 JLINK_GetId() >0x0D TIF> >0x21 TIF>  returns 0x1BA01477 (0002ms, 0265ms total)
T0BD0 000:457 JLINK_GetFirmwareString(...) (0000ms, 0265ms total)
T0BD0 004:133 JLINK_IsOpen()  returns 0x01 (0000ms, 0266ms total)
T0BD0 004:133 JLINK_Close() >0x42 TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> (0067ms, 0333ms total)
T0BD0 004:202 JLINK_SelectUSB(Port = 0)  returns 0x00 (0000ms, 0333ms total)
T0BD0 004:202 JLINK_EnableLog(...) (0000ms, 0333ms total)
T0BD0 004:202 JLINK_SetWarnOutHandler(...) (0000ms, 0333ms total)
T0BD0 004:202 JLINK_OpenEx(...)
Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
Hardware: V7.00
S/N: 20090928
Feature(s): RDI,FlashDL,FlashBP,JFlash,GDBFull  returns O.K. (0029ms, 0362ms total)
T0BD0 004:231 JLINK_SetErrorOutHandler(...) (0000ms, 0362ms total)
T0BD0 004:232 JLINK_ExecCommand("ProjectFile = "F:\佳显电子\新产品开发\新产品开发--合力泰电子纸\常规品\GDEH0116Zx_SSD1677-20200309\Project\JLinkSettings.ini"", ...)  returns 0x00 (0001ms, 0363ms total)
T0BD0 004:233 JLINK_ExecCommand("Device = STM32F103VE", ...)
                JLINK_AddMirrorAreaEx(Addr = 0x00000000, Size = 0x00000000) (0001ms, 0001ms total)
              Device "STM32F103VE" selected (512 KB flash, 64 KB RAM).  returns 0x00 (0002ms, 0365ms total)
T0BD0 004:235 JLINK_ExecCommand("DisableConnectionTimeout", ...)  returns 0x01 (0000ms, 0365ms total)
T0BD0 004:235 JLINK_GetHardwareVersion()  returns 0x11170 (0000ms, 0365ms total)
T0BD0 004:235 JLINK_GetDLLVersion()  returns 47604 (0000ms, 0365ms total)
T0BD0 004:235 JLINK_GetFirmwareString(...) (0000ms, 0365ms total)
T0BD0 004:235 JLINK_GetDLLVersion()  returns 47604 (0000ms, 0365ms total)
T0BD0 004:235 JLINK_GetCompileDateTime() (0000ms, 0365ms total)
T0BD0 004:235 JLINK_GetFirmwareString(...) (0000ms, 0365ms total)
T0BD0 004:235 JLINK_GetHardwareVersion()  returns 0x11170 (0000ms, 0365ms total)
T0BD0 004:235 JLINK_TIF_Select(JLINKARM_TIF_JTAG)  returns 0x00 (0000ms, 0365ms total)
T0BD0 004:235 JLINK_SetSpeed(5000) (0001ms, 0366ms total)
T0BD0 004:236 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)  returns JLINKARM_RESET_TYPE_NORMAL (0000ms, 0366ms total)
T0BD0 004:236 JLINK_Reset() >0x2F8 JTAG>Could not measure total IR len. TDO is constant high. >0x30 JTAG>STM32F1xxx: Can not attach to CPU. Trying connect under reset. >0x2F8 JTAG>Could not measure total IR len. TDO is constant high. >0x30 JTAG>JLINK_GetIdData(...) >0x2F8 JTAG>Could not measure total IR len. TDO is constant high. >0x30 JTAG>STM32F1xxx: Can not attach to CPU. Trying connect under reset. >0x2F8 JTAG>Could not measure total IR len. TDO is constant high. >0x30 JTAG> (0112ms, 0590ms total)
T0BD0 004:460 JLINK_GetIdData(...) >0x2F8 JTAG>Could not measure total IR len. TDO is constant high. >0x30 JTAG>STM32F1xxx: Can not attach to CPU. Trying connect under reset. >0x2F8 JTAG>Could not measure total IR len. TDO is constant high. >0x30 JTAG> (0112ms, 0702ms total)
T0BD0 004:576 JLINK_GetFirmwareString(...) (0000ms, 0702ms total)
T0BD0 006:181 JLINK_IsOpen()  returns 0x01 (0000ms, 0702ms total)
T0BD0 006:181 JLINK_Close() (0057ms, 0759ms total)
T0BD0 006:241 JLINK_SelectUSB(Port = 0)  returns 0x00 (0000ms, 0759ms total)
T0BD0 006:241 JLINK_EnableLog(...) (0000ms, 0759ms total)
T0BD0 006:241 JLINK_SetWarnOutHandler(...) (0000ms, 0759ms total)
T0BD0 006:241 JLINK_OpenEx(...)
Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
Hardware: V7.00
S/N: 20090928
Feature(s): RDI,FlashDL,FlashBP,JFlash,GDBFull  returns O.K. (0029ms, 0788ms total)
T0BD0 006:270 JLINK_SetErrorOutHandler(...) (0000ms, 0788ms total)
T0BD0 006:271 JLINK_ExecCommand("ProjectFile = "F:\佳显电子\新产品开发\新产品开发--合力泰电子纸\常规品\GDEH0116Zx_SSD1677-20200309\Project\JLinkSettings.ini"", ...)  returns 0x00 (0001ms, 0789ms total)
T0BD0 006:272 JLINK_ExecCommand("Device = STM32F103VE", ...)
                JLINK_AddMirrorAreaEx(Addr = 0x00000000, Size = 0x00000000) (0001ms, 0001ms total)
              Device "STM32F103VE" selected (512 KB flash, 64 KB RAM).  returns 0x00 (0002ms, 0791ms total)
T0BD0 006:274 JLINK_ExecCommand("DisableConnectionTimeout", ...)  returns 0x01 (0000ms, 0791ms total)
T0BD0 006:274 JLINK_GetHardwareVersion()  returns 0x11170 (0000ms, 0791ms total)
T0BD0 006:274 JLINK_GetDLLVersion()  returns 47604 (0000ms, 0791ms total)
T0BD0 006:274 JLINK_GetFirmwareString(...) (0000ms, 0791ms total)
T0BD0 006:274 JLINK_GetDLLVersion()  returns 47604 (0000ms, 0791ms total)
T0BD0 006:274 JLINK_GetCompileDateTime() (0000ms, 0791ms total)
T0BD0 006:274 JLINK_GetFirmwareString(...) (0000ms, 0791ms total)
T0BD0 006:274 JLINK_GetHardwareVersion()  returns 0x11170 (0000ms, 0791ms total)
T0BD0 006:274 JLINK_TIF_Select(JLINKARM_TIF_SWD)  returns 0x00 (0004ms, 0795ms total)
T0BD0 006:278 JLINK_SetSpeed(5000) (0001ms, 0796ms total)
T0BD0 006:281 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)  returns JLINKARM_RESET_TYPE_NORMAL (0000ms, 0796ms total)
T0BD0 006:281 JLINK_Reset() >0x108 TIF>Found SWD-DP with ID 0x1BA01477 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x108 TIF>Found SWD-DP with ID 0x1BA01477 >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>
 >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>Found Cortex-M3 r1p1, Little endian. -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE0002000)FPUnit: 6 code (BP) slots and 2 literal slots
 -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_ReadMem(4 bytes @ 0xE00FF010)TPIU fitted. -- CPU_ReadMem(4 bytes @ 0xE00FF014)ETM fitted. -- CPU_ReadMem(4 bytes @ 0xE00FF018) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC) >0x35 TIF> -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000ED0C) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running
 -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000) (0101ms, 0897ms total)
T0BD0 006:382 JLINK_GetId() >0x0D TIF> >0x21 TIF>  returns 0x1BA01477 (0003ms, 0900ms total)
T0BD0 006:389 JLINK_GetFirmwareString(...) (0000ms, 0900ms total)
T0BD0 007:868 JLINK_IsOpen()  returns 0x01 (0000ms, 0900ms total)
T0BD0 007:868 JLINK_Close() >0x42 TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> (0049ms, 0949ms total)
T0BD0 007:919 JLINK_SelectUSB(Port = 0)  returns 0x00 (0000ms, 0949ms total)
T0BD0 007:919 JLINK_EnableLog(...) (0000ms, 0949ms total)
T0BD0 007:919 JLINK_SetWarnOutHandler(...) (0000ms, 0949ms total)
T0BD0 007:919 JLINK_OpenEx(...)
Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
Hardware: V7.00
S/N: 20090928
Feature(s): RDI,FlashDL,FlashBP,JFlash,GDBFull  returns O.K. (0030ms, 0979ms total)
T0BD0 007:949 JLINK_SetErrorOutHandler(...) (0000ms, 0979ms total)
T0BD0 007:951 JLINK_ExecCommand("ProjectFile = "F:\佳显电子\新产品开发\新产品开发--合力泰电子纸\常规品\GDEH0116Zx_SSD1677-20200309\Project\JLinkSettings.ini"", ...)  returns 0x00 (0000ms, 0979ms total)
T0BD0 007:951 JLINK_ExecCommand("Device = STM32F103VE", ...)
                JLINK_AddMirrorAreaEx(Addr = 0x00000000, Size = 0x00000000) (0000ms, 0000ms total)
              Device "STM32F103VE" selected (512 KB flash, 64 KB RAM).  returns 0x00 (0003ms, 0982ms total)
T0BD0 007:954 JLINK_ExecCommand("DisableConnectionTimeout", ...)  returns 0x01 (0000ms, 0982ms total)
T0BD0 007:954 JLINK_GetHardwareVersion()  returns 0x11170 (0000ms, 0982ms total)
T0BD0 007:954 JLINK_GetDLLVersion()  returns 47604 (0000ms, 0982ms total)
T0BD0 007:954 JLINK_GetFirmwareString(...) (0000ms, 0982ms total)
T0BD0 007:954 JLINK_GetDLLVersion()  returns 47604 (0000ms, 0982ms total)
T0BD0 007:954 JLINK_GetCompileDateTime() (0000ms, 0982ms total)
T0BD0 007:954 JLINK_GetFirmwareString(...) (0000ms, 0982ms total)
T0BD0 007:954 JLINK_GetHardwareVersion()  returns 0x11170 (0000ms, 0982ms total)
T0BD0 007:955 JLINK_TIF_Select(JLINKARM_TIF_SWD)  returns 0x00 (0004ms, 0986ms total)
T0BD0 007:959 JLINK_SetSpeed(3000) (0001ms, 0987ms total)
T0BD0 007:961 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)  returns JLINKARM_RESET_TYPE_NORMAL (0000ms, 0987ms total)
T0BD0 007:961 JLINK_Reset() >0x108 TIF>Found SWD-DP with ID 0x1BA01477 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x108 TIF>Found SWD-DP with ID 0x1BA01477 >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>
 >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>Found Cortex-M3 r1p1, Little endian. -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE0002000)FPUnit: 6 code (BP) slots and 2 literal slots
 -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_ReadMem(4 bytes @ 0xE00FF010)TPIU fitted. -- CPU_ReadMem(4 bytes @ 0xE00FF014)ETM fitted. -- CPU_ReadMem(4 bytes @ 0xE00FF018) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC) >0x35 TIF> -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000ED0C) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running
 -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000) (0099ms, 1086ms total)
T0BD0 008:060 JLINK_GetId() >0x0D TIF> >0x21 TIF>  returns 0x1BA01477 (0003ms, 1089ms total)
T0BD0 008:067 JLINK_GetFirmwareString(...) (0000ms, 1089ms total)
T0BD0 011:596 JLINK_SWO_Control(JLINKARM_SWO_CMD_GET_SPEED_INFO, ...)  returns 0x00 (0002ms, 1091ms total)
T0BD0 011:598 JLINK_SWO_Control(JLINKARM_SWO_CMD_GET_SPEED_INFO, ...)  returns 0x00 (0002ms, 1093ms total)
T0BD0 011:600 JLINK_SWO_Control(JLINKARM_SWO_CMD_GET_SPEED_INFO, ...)  returns 0x00 (0002ms, 1095ms total)
T0BD0 011:602 JLINK_SWO_Control(JLINKARM_SWO_CMD_GET_SPEED_INFO, ...)  returns 0x00 (0002ms, 1097ms total)
T0BD0 011:604 JLINK_SWO_Control(JLINKARM_SWO_CMD_GET_SPEED_INFO, ...)  returns 0x00 (0002ms, 1099ms total)
T0BD0 011:606 JLINK_SWO_Control(JLINKARM_SWO_CMD_GET_SPEED_INFO, ...)  returns 0x00 (0002ms, 1101ms total)
T0BD0 011:608 JLINK_SWO_Control(JLINKARM_SWO_CMD_GET_SPEED_INFO, ...)  returns 0x00 (0002ms, 1103ms total)
T0BD0 011:610 JLINK_SWO_Control(JLINKARM_SWO_CMD_GET_SPEED_INFO, ...)  returns 0x00 (0002ms, 1105ms total)
T0BD0 011:612 JLINK_SWO_Control(JLINKARM_SWO_CMD_GET_SPEED_INFO, ...)  returns 0x00 (0002ms, 1107ms total)
T0BD0 011:615 JLINK_SWO_Control(JLINKARM_SWO_CMD_GET_SPEED_INFO, ...)  returns 0x00 (0003ms, 1110ms total)
T0BD0 013:291 JLINK_Close() >0x42 TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> (0050ms, 1160ms total)
T0BD0 013:344 JLINK_Close() (0001ms, 1162ms total)
T0BD0 013:348 JLINK_Close() (0000ms, 1162ms total)
